**Card-1 & Card-2:**

GPS+AGPS+LBS positioning

Allow the location to be pinpointed accurately and rapidly

Auto-mute mode on classesNever disturb the classes via auto-setting

Geo-fence alarm

Create geofences in circle or rectangle for key locations

Voice monitor

Activate listen-in mode via text

SOS call & Speed-dial

 In case of emergency, press the SOS button to trigger an urgent call

White list

Only authorized numbers could call in

Low battery & Shutdown

noticeReceive notice when the phone needs for charging

Tracked by: SMS, APP, Web Reports location In real time through different interfaces

**LDO2**

**Feature**

**Light and compact**

**Small size allowing covert & easy mounting**

**GPS positioning**

**Allow the location to be pinpointed in real time or periodically**

**Built-in GPS & GSM antennaSuperior sensitivity and fast time for first fixEasy installation Plug-and-track, easy to swap between vehicles**

**Intelligent power management**

**Reduce power consumption when device stays idle**

**Configure alerts for over-speeding**

**Send instant email/SMSto notify vehicle`s speeding**

**Driving history record**

**Review a vehicle`s history and activity throughout the day through web**

**Tracked by: SMS, APP, Web Reports iocation in real time through different interfaces**

**LD06N**

**LD06N The World's Most Popular GPS Tracking Device**

**Afteryears of popularity around the globe, LD06N has earned its market-proven stability and durability. Loaded with features, the battery-powered LD06N gives you real-time location viewing from the comfort of your computer or smartphone, and makes it a prefect choice for private cars and fleet management.**

**Feature**

**Remote cut-off (petrol/power)**

**Compel the vehicle to stop by breaking off the fuel connection**

**Bullt-in 450mAh battery**

**High capacity Li-ion battery ensuring sufficlent power supply**

**ACC detection for ignition status**

**Be aware of the ignition status whenever you need**

**SOS emergency call**

**Thumb sized button allowing urgent call during an emergency case**

**Configurable tracking modes**

**Location uploaded following fixed distance,time interval, preset cornering**

**Multiple alarms**

**Instant alert for vibration, overspeed. power off, geo-fence**

**Volce monitor**

**Activate listen-in mode via text**

**Tracked by: SMS, APP, Web Reports location in real time through different interfaces**

**LDTrack2**

**LDTrack2 General GPS Vehicle Tracker**

**LDTrack2 GPS vehicle tracker is designed to meet the needs of various peripherals. Its wide voltage range ensures its stable running on electromobiles, motorcycles, cars and trucks. Small but compact, its highly reliable electric circuit and internal battery designfunctions not only basic tracking butSOS call, tele-cutoff fuel, geo-fence, overspeedalert, historical data upload and more.**

**Feature**

**Remote cut-off (petrol/power)**

**Compel the vehicle to stop by breaking off the fuel connection**

**Light and compactSmall size allowing covert & easy mounting**

**ACC detection for lgnition status Be aware of the igniton status whenever you need**

**9-90V voltage range**

**Wide operating voltage applicable to all types of vehicles**

**Configurable fracking modes**

**Location uploaded following fixed distance, time interval, preset cornering**

**Multiple alarms**

**Instant alert for vibration, overspeed, power off, geo-fenceVehicle battery protection**

**Never drain out of the battery of moforcycle for optimal protection**

**Tracked by: SMS, APP, Web Reports location in real time through different interfaces**

**LD800**

**LD800 Vehicle GPS Tracker is a high-end multifunctional vehicle GPS tracker with solid performance for reasonable price. In addition to GPS and AGPS tracking, This GPS tracker device supports door status detection, two-way communication as well as SOS call.**

**Feature**

**GPS+AGPS**

**tracking Allow the location to be pinpointed in real time or periodically**

**IP66 dust and waterproof**

**Water-resistant to ensure stable operation in tough environment**

**50000 pieces of data storage**

**Memorize a large amount of gps data for history review**

**Door status detection**

**Get instant alert when your car's door is open expectedly**

**SOS emergency**

**callIng case of emergency,press the SOS button to trigger an urgent callTwo-way communicationWith MIC and speaker connected, it's easy to realize voice-monitor or two-way audio**

**Multiple analog & digital I/O**

**Monitor and control external application via inputs/outputs**

**Multiple alarms**

**Instant alert for vibration, overspeed, power off, geo-fence**